Setup Jetson Nano

Connect your Nano with screen and keyboard

nano pwd: arg

nano $ sudo vim /etc/hostname

change the robot name into your robot name

nano $ sudo vim /etc/hosts

change the robot name into your robot name

nano $ sudo reboot

How to connect Jetson Nano with vncviewer

laptop $ ssh arg@[nano\_name].local

nano $ export DISPLAY=:0 && xrandr --fb 1800x900

nano $ /usr/lib/vino/vino-server

laptop $ vncviewer -quality 0 -encodings "tight" [nano\_name].local